2021 Logger Run Notes:

Saved Hobo files to two locations on my comp (for data security)

One in folder on desktop, one under my documents>HOBOware folder

1-19-21

**Dry Spottedtail\_Steffl**

Same location. Wrapped around gauge height meter under bridge (intersection of CR 13 and CR E).

41.94267, -103.83308 pt 587

**Sheep\_Site1- not downloaded**

Attached to green T-post on east side of stream, just downstream of overhanging tree.

42.04888, -104.02879

**Sheep\_Site2**

Pulled logger and did not redeploy

1-20-21

White\_Andrews

Could not find(2017-2018 data). New logger placed on west side of road near culvert. Logger should be right in front of the height gauge by culvert, may get a little silted in due to run off from road? Used a T post as to secure wire. 42.63010, -103.73568

Coffee Park

Placed at first fence crossing below the parking lot. Right bank looking downstream, the wire is attached to a tree root. Rocks placed over the casing.

42.73421, -103.84023

Monroe

Placed in same pool as usual. Between 1st and 2nd bend downstream the small atv crossing. T-post placed to mark location. Rebar/logger pushed into undercut area.

42.76742,-103.92763 pt 590

Squaw – lost did not redeploy

WestAsh- pulled logger, did not redeploy

East Ash – pulled logger, did not redeploy

Bordeaux- North –Same location by the tree

Bordeaux Cliffs same location below culvert attached to tree

Pine- north attached to culvert staked at the bottom left mouth of culvert.42.48635,-103.43787 pt 591